Link: amazon.com/gp/product/B07NQJ1VZ2/ref=ppx\_yo\_dt\_b\_asin\_title\_o09\_s01?ie=UTF8&psc=1

Gear Type: All Metal Gears

Connector Wire :11.81 inch (300mm),

signal wire/PWM--Yellow;

positive Pole(+)--Red;

negative Pole/GND(-)—Brown

Item Dimension:40.7\*19.7\*42.9mm(1.60\*0.78\*1.69inch)

Servo Weight: 55g

Positioning speed at 4.8V without load0.17s / 60 degrees; 6.0V without load 0.13s / 60 degrees

Dead Band Width: 4us

Plug Specification: JR FUTABA, Hitec,Sanwa, GWS are universal

Operation Voltage: 3.0V - 7.2V

Stall torque: 6V 12kg/cm, 7.2V 13kg/cm.

Temperature range: -30 to +60deg

Applicable models: biped robot / robot / remote control car, suitable for50-90 methanol fixed-wing aircraft and  
    26cc-50ccgasoline fixed-wing aircraft and other models

Accessories; steering wheel, fixing screws, rubber sleeves and aluminumsleeves.

Suitable for most receiver connector: Futaba, Hitec, Sanwa, GWS etc

Great for truck, Boat, Racing Car,Helicopter and Airplane.

**Package includes:**

4Pcs MG995 HI-SPEED RC Servo Motor;  
Servo HornKit