Maximum force experienced across the valve before movement in wet and dry condition were largely the same.

Force: .5 lbf

Moment Arm: 4 inches

Moment = 2 in\*lbf

“= 0.226 N-m

“=2.304 kg\*cm